Joshua Spisak

CS 447 – Lab 3-b

January 28, 2019

B.1 0x1d1c1b1a

B.2 The address of the byte containing 0x1b is 0x10010001

B.3 0x1a1b1c1d

B.4 The byte with the most value is 0x1a

B.5 The byte with the highest address is also 0x1a

B.6 The simulator is little-endian because the least significant bit has the smallest address.